XY-1B1BF series precision balance

Function

★ LCD/AC and DC power supply（AA*3）

★ Tare function/Counting/Unit conversion (g/ct/oz)...

★ Min weighing set

★ Overload alarm/Level indicator

★ Option:Dual display/Interface/Printer/Windproof/Dust cover

	XY-2C Specifications 

	Model
	Capacity
	Readability
	Repeatability
	Linearity
	Pan Size
	Stable Time

	XY100-2C
	110g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY200-2C
	210g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY300-2C
	310g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY500-2C
	510g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY600-2C
	610g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY1000-2C
	1100g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY2000-2C
	2100g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S

	XY3000-2C
	3100g
	0.01g
	±0.02g
	±0.03g
	Ø130mm
	≤2S


 
